Lab - Identify IPv6 Addresses

# Topology



# Objectives

Part 1: Practice with Different Types of IPv6 Addresses

Part 2: Examine a Host IPv6 Network Interface and Address

# Background / Scenario

With the depletion of the Internet Protocol version 4 (IPv4) network address space and the adoption and transition to IPv6, networking professionals must understand how both IPv4 and IPv6 networks function. Many devices and applications already support IPv6. This includes extensive Cisco device Internetwork Operating System (IOS) support and workstation/server operating system support, such as that found in Windows and Linux.

This lab focuses on IPv6 addresses and the components of the address. In Part 1, you will identify the IPv6 address types and IPv6 addresses abbreviation. In Part 2, you will view the IPv6 settings on a PC.

# Required Resources

* 1 PC (Windows with internet access)

# Instructions

## Practice with Different Types of IPv6 Addresses

In this part, you will identify the different types of IPv6 addresses and practice compressing and decompressing IPv6 addresses.

### Match the IPv6 address to its type.

Match the IPv6 addresses to their corresponding address type. Notice that the addresses have been compressed to their abbreviated notation and that the slash network prefix number is not shown. Some answer choices must be used more than once.

Answer choices:

* + - 1. Loopback address
      2. Global unicast address
      3. Link-local address
      4. Unique-local address
      5. Multicast address

| IPv6 Address | Answer |
| --- | --- |
| 2001:0db8:1:acad::fe55:6789:b210 | blank |
| ::1 | blank |
| fc00:22:a:2::cd4:23e4:76fa | blank |
| 2033:db8:1:1:22:a33d:259a:21fe | blank |
| fe80::3201:cc01:65b1 | blank |
| ff00:: | blank |
| ff00::db7:4322:a231:67c | blank |
| ff02::2 | blank |

### Practice compressing and decompressing IPv6 addresses.

#### Questions:

Using the rules of IPv6 address abbreviation, either compress or decompress the following addresses:

2002:0ec0:0200:0001:0000:04eb:44ce:08a2

Type your answers here.

fe80:0000:0000:0001:0000:60bb:008e:7402

Type your answers here.

fe80::7042:b3d7:3dec:84b8

Type your answers here.

ff00::

Type your answers here.

2001:0030:0001:acad:0000:330e:10c2:32bf

Type your answers here.

## Examine a Host IPv6 Network Interface and Address

In Part 2, you will check the IPv6 network settings of your PC to identify your network interface IPv6 address.

### Check your PC IPv6 network address settings.

Verify that the IPv6 protocol is installed and active on your PC-A (check your Local Area Connection settings).

* + - 1. Navigate to the **Control Panel**.
      2. In the Category View, click **Network and Sharing Center** icon. Click **View network status and tasks**.
      3. In the Network and Sharing Center window, you will see your active networks.
      4. On the left side of the window, click **Change adapter settings**. You should now see icons representing your installed network adapters. Right-click your active network interface (it may be an **Ethernet** or a **Wi-Fi**), and then click **Properties**.
      5. In the Properties window, scroll through the list of items to determine whether IPv6 is present, which indicates that it is installed, and if it is also check marked, which indicates that it is active.
      6. Select the item **Internet Protocol Version 6 (TCP/IPv6)** and click **Properties**. You should see the IPv6 settings for your network interface. Your IPv6 properties window is likely set to **Obtain an IPv6 address automatically**. This does not mean that IPv6 relies on the Dynamic Host Configuration Protocol (DHCP). Instead of using DHCP, IPv6 looks to the local router for IPv6 network information and then auto-configures its own IPv6 addresses. To manually configure IPv6, you must provide the IPv6 address, the subnet prefix length, and the default gateway. Click **Cancel** to exit the properties windows.

**Note**: The local router can refer host requests for IPv6 information, especially Domain Name System (DNS) information, to a DHCPv6 server on the network.

* + - 1. After you have verified that IPv6 is installed and active on your PC, you should check your IPv6 address information.

### Verify the IPv6 address settings using the Command Prompt.

* + - 1. Open a command prompt and enter the **ipconfig /all** command. Your output should look similar to this:

C:\Users\user> **ipconfig /all**

Windows IP Configuration

<output omitted>

Wireless LAN adapter Wireless Network Connection:

Connection-specific DNS Suffix . :

Description . . . . . . . . . . . : Intel(R) Centrino(R) Advanced-N 6200 AGN

Physical Address. . . . . . . . . : 02-37-10-41-FB-48

DHCP Enabled. . . . . . . . . . . : Yes

Autoconfiguration Enabled . . . . : Yes

**Link-local IPv6 Address . . . . . : fe80::8d4f:4f4d:3237:95e2%14(Preferred)**

IPv4 Address. . . . . . . . . . . : 192.168.2.106(Preferred)

Subnet Mask . . . . . . . . . . . : 255.255.255.0

Lease Obtained. . . . . . . . . . : Sunday, January 06, 2013 9:47:36 AM

Lease Expires . . . . . . . . . . : Monday, January 07, 2013 9:47:38 AM

Default Gateway . . . . . . . . . : 192.168.2.1

DHCP Server . . . . . . . . . . . : 192.168.2.1

DHCPv6 IAID . . . . . . . . . . . : 335554320

DHCPv6 Client DUID. . . . . . . . : 00-01-00-01-14-57-84-B1-1C-C1-DE-91-C3-5D

DNS Servers . . . . . . . . . . . : 192.168.1.1

8.8.4.4

<output omitted>

* + - 1. You can see from the output that the client PC has an IPv6 link-local address with a randomly generated interface ID.

#### Questions:

What does it indicate about the network regarding IPv6 global unicast address, IPv6 unique-local address, or IPv6 gateway address?

Type your answers here.

What kind of IPv6 addresses did you find when using **ipconfig /all**?

Type your answers here.

# Reflection Questions

* 1. How do you think you must support IPv6 in the future?

Type your answers here.

* 1. Do you think IPv4 networks continue on, or will everyone eventually switch over to IPv6? How long do you think it will take?

Type your answers here.

# Answer Key

## Practice with Different Types of IPv6 Addresses

### Match the IPv6 address to its type.

Answer choices:

* + - 1. Loopback address
      2. Global unicast address
      3. Link-local address
      4. Unique-local address
      5. Multicast address

| IPv6 Address | Answer |
| --- | --- |
| 2001:0db8:1:acad::fe55:6789:b210 | B |
| ::1 | A |
| fc00:22:a:2::cd4:23e4:76fa | D |
| 2033:db8:1:1:22:a33d:259a:21fe | B |
| fe80::3201:cc01:65b1 | C |
| ff00:: | E |
| ff00::db7:4322:a231:67c | E |
| ff02::2 | E |

### Practice compressing and decompressing IPv6 addresses.

2002:0ec0:0200:0001:0000:04eb:44ce:08a2

2002:ec0:200:1::4eb:44ce:8a2

fe80:0000:0000:0001:0000:60bb:008e:7402

fe80::1:0:60bb:8e:7402

fe80::7042:b3d7:3dec:84b8

fe80:0000:0000:0000:7042:b3d7:3dec:84b8

ff00::

ff00:0000:0000:0000:0000:0000:0000:0000

2001:0030:0001:acad:0000:330e:10c2:32bf

2001:30:1:acad::330e:10c2:32bf

## Examine a Host IPv6 Network Interface and Address

In Part 2, you will check the IPv6 network settings of your PC to identify your network interface IPv6 address.

### Check your PC IPv6 network address settings.

### Verify the IPv6 address settings using the Command Prompt.

What does it indicate about the network regarding IPv6 global unicast address, IPv6 unique-local address, or IPv6 gateway address?

It indicates that there is no IPv6 enabled gateway router providing global address, local address, or subnet information on the network.

What kind of IPv6 addresses did you find when using **ipconfig /all**?

Answers will vary, but most likely they will be link-local addresses also.

# Reflection Questions

* 1. How do you think you must support IPv6 in the future?

Answers will vary. A sample answer: Future devices should support IPv6 because IPv6 will eventually replace IPv4. IPv6 also simplifies and speeds up data transmission. Furthermore, IPv6 was built with security in mind. By default, IPv6 encrypts traffic and check packet integrity.

* 1. Do you think IPv4 networks continue on, or will everyone eventually switch over to IPv6? How long do you think it will take?

Answers will vary. A sample answer: The IPv6 adoption will continue while IPv4 network continues to support IPv4 user devices. It is still a long time before everyone switches over to IPv6 completely. This link provides some insight into the IPv6 capable by country: <https://stats.labs.apnic.net/ipv6>.

End of document